**Check cap orientation (red stripe down)**

**Apply USB power**

**Keyboard to Hub MIDI input**

**Hub MIDI output 1 to PC input**

**Play notes on keyboard and use MIDI-OX to check input**

**Check LEDs beside MIDI input blink with traffic**

**Press START and check that all LEDs function**

**Check MIDI clock messages received**

**Press STOP – START and check for MIDI stop/start**

**Check 120BPM when running**

**Press ++ ten times and check 130BPM**

**Press ++ and -- together and check for 120BPM**

**Press -- ten times and check 110BPM**

**Use each MIDI output and check clock messages are passed**